|  |  |
| --- | --- |
| Mobile Equip - Tipping Vehicle Operation |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name:** |  | **Date:** |  |
| **Job Description:** |  | **Location:** |  |

# Performance Metrics

|  |  |  |  |
| --- | --- | --- | --- |
|  | ✓ | 🗶 | • |
| Tipping operations conducted on stable, firm level ground. |  |  |  |
| Tipping not permitted in the open during adverse weather e.g. high cross winds that can lead to instability of raised tipping body. |  |  |  |
| Operators trained in conducting tipping vehicle operations. With tipping vehicle operated within technical capabilities and limitations of the vehicle for the load/ weight distribution. |  |  |  |
| Driver in a safe position e.g. at the rear of load at sufficient distance to be clear of any material spills from tipping body and monitoring the discharge. No personnel standing beside a raised tipping body. |  |  |  |

# Supervisor Task Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Provide and maintain firm, level, stable ground to conduct tipping operations. |  |  |  |
| Verify that any person required to conduct tipping operations is trained and assessed competent in conduct of those operations. |  |  |  |
| Direct tipping operations to cease in adverse weather conditions if there is a risk to stability of raised tipping body (e.g. high cross winds). |  |  |  |

# Operator / Maintainer Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Apply brakes and set wheel chocks on tipping vehicle. |  |  |  |
| Monitor discharge from safe position. Do not stand beside a raised tipping body. |  |  |  |
| Unload tipping body in several stages. Do not completely raise the tipping body when full. Raise tipping hoist to highest level in several steps. |  |  |  |
| Operate tipping vehicle within technical capabilities and limitations of the vehicle for the load/ weight distribution. |  |  |  |
| Never drive a vehicle with the tipping body raised. Lower the tipping body completely after discharge confirmed as complete before driving away. |  |  |  |
| Stop tipping operations in adverse weather conditions if there is a risk to stability of raised tipping body (e.g. high cross winds). Lower tipping body. |  |  |  |
| Maintain tipping equipment fit for purpose as per manufacturers’ recommendation. |  |  |  |
| Stop work if personnel enter exclusion zone under suspended load. |  |  |  |

# Comments/Actions