|  |  |
| --- | --- |
| Suspended Baskets Or Cages |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name:** |  | **Date:** |  |
| **Job Description:** |  | **Location:** |  |

# Performance Metrics

|  |  |  |  |
| --- | --- | --- | --- |
|  | ✓ | 🗶 | • |
| Lifting equipment (including fixed or mobile crane, basket, cage etc.) is designed in accordance with recognised standards and / or hired from an established, reputable company. |  |  |  |
| Separate baskets / man-cage attachments, used in conjunction with lifting equipment to suspend persons, are designed in accordance with recognised standards and subject to a planned maintenance and inspection program. |  |  |  |
| Baskets / cage attachments are fitted with an approved anchor point. |  |  |  |
| People involved in directing the operation of lifting equipment (e.g. Rigger, Dogman etc.) are trained and assessed as competent in the requirements of the activity, including holding any licence / permit required by local regulations. |  |  |  |
| Lifting equipment is stabilised in accordance with the manufacturer's instructions before use (e.g. ground area supporting lifting equipment prepared, crane pads used, outriggers used). |  |  |  |
| Suspended baskets or cages are used as working platforms only, not as a means of entering or exiting a work area. |  |  |  |
| Lifting equipment is subject to a planned maintenance and inspection program in accordance with recognised standards and the manufacturer's recommendations. |  |  |  |
| Lifting equipment, including ropes, wires and slings, are inspected by a third-party specialist in accordance with local regulations. |  |  |  |
| People required to operate lifting equipment (e.g. cranes) are trained and assessed as competent in the set-up and operation of the equipment, including holding any licence / permit required by local regulations. |  |  |  |
| Fall protection equipment, consisting of a harness and fixed-length lanyard, is worn and attached to the approved anchor point whilst working from the suspended basket or cage. |  |  |  |
| An exclusion zone is established around the lifting equipment, including barricades, signs and an observer, to prevent third party access. |  |  |  |

# Supervisor Task Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Verify hired lifting equipment has been sourced from approved, reputable companies. |  |  |  |
| Verify that OTML owned lifting equipment, along with any separate basket / man-cage attachment, has been inspected and maintained in accordance with the established program. |  |  |  |
| Verify that the maintenance records of any hired lifting equipment are available with the equipment, and have been checked. |  |  |  |
| Verify that any person required to work from a suspended basket has been trained and assessed competent in working at height. |  |  |  |
| Verify that any person operating or directing lifting equipment has been trained and assessed competent in its use, including holding any required licence or permit. |  |  |  |
| Verify any basket / man-cage attachment is fitted with an approved anchor point. |  |  |  |

# Operator / Maintainer Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Operate or direct lifting equipment only if trained and authorised for this activity. |  |  |  |
| Stabilise the lifting equipment before use in accordance with the manufacturer's instructions (e.g. ground area supporting lifting equipment adequately prepared, crane pads used, outriggers in place). |  |  |  |
| Establish an exclusion zone around the lifting equipment, including barricades, signs and an observer, before operating the equipment. |  |  |  |
| Inspect condition of lifting equipment before use and report any substandard condition to the relevant supervisor. |  |  |  |
| Wear fall protection equipment, attached to an approved anchor point, when working from a suspended basket. |  |  |  |
| Do not exit the work basket or man-cage during the work activity at height. |  |  |  |

# Comments/Actions