|  |  |
| --- | --- |
| Working from Elevated Fixed Structures - Integrity of Structure |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name:** |  | **Date:** |  |
| **Job Description:** |  | **Location:** |  |

# Performance Metrics

|  |  |  |  |
| --- | --- | --- | --- |
|  | ✓ | 🗶 | • |
| Fixed platforms, walkways, stairways and handrails are designed to support people safely in accordance with recognised standards. |  |  |  |
| Civil and structural equipment, including support beams and columns, are subject to a planned maintenance and inspection program. |  |  |  |
| The load bearing capacity of any fixed structure not designed as a workplace (e.g. roof, suspended ceiling etc.) is assessed and approved by a structural engineer before structure is accessed. |  |  |  |
| Fixed platforms, walkways, stairways and handrails are subject to a planned maintenance and inspection program. |  |  |  |
| Civil and structural equipment, including support beams and columns, are audited by a qualified, independent third party according to local regulations. |  |  |  |
| Signs are in place at likely access points to any fixed structure not designed as a workplace (e.g. roof, suspended ceiling etc.), indicating a fragile structure and prohibiting access without a Work at Heights permit. |  |  |  |

# Supervisor Task Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Provide trained resources to maintain and assess elevated fixed structures. |  |  |  |
| Verify that elevated fixed structures have been inspected and maintained in accordance with the established program. |  |  |  |
| Verify the load bearing capacity of any fixed structure not designed as a workplace (e.g. roof, suspended ceiling etc.) has been assessed and approved by a structural engineer before the structure is accessed. |  |  |  |
| Provide signs, at likely access points to any fixed structure not designed as a workplace, prohibiting access without a Work at Heights permit. |  |  |  |

# Operator / Maintainer Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Report any substandard structural condition to a relevant supervisor. Do not proceed to access the structure until the condition is rectified. |  |  |  |
| Do not access any elevated structure that is not intended as a place of work, including any structure with signage indicating no access, unless a Work at Heights permit has been issued. |  |  |  |

# Comments/Actions