|  |  |
| --- | --- |
| Use of Split Rims on Mobile Equipment |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name:** |  | **Date:** |  |
| **Job Description:** |  | **Location:** |  |

# Performance Metrics

|  |  |  |  |
| --- | --- | --- | --- |
|  | ✓ | 🗶 | • |
| Non-pneumatic puncture proof tyres are used with split or divided rims. These tyres are of a solid construction relying on the flexibility of the material from which they are constructed. They do not have valve stems. Some have holes in the side wall.  |  |  |  |

# Supervisor Task Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Ensure mobile equipment with spilt rims are fitted with non-pneumatic puncture proof tyres.  |  |  |  |

# Operator / Maintainer Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| NA. |  |  |  |

# Comments/Actions