|  |  |
| --- | --- |
| Securing Items To Vehicles and Mobile Equipment |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name:** |  | **Date:** |  |
| **Job Description:** |  | **Location:** |  |

# Performance Metrics

|  |  |  |  |
| --- | --- | --- | --- |
|  | ✓ | 🗶 | • |
| Items (e.g. boom, hose reel, etc.) are secured in home position within the chassis line of the vehicle by a fitted secondary restraint, unless in use. |  |  |  |
| Fire extinguishers are secured in carriers / to mounting brackets by secondary restraint (which can easily and quickly be released in an emergency). |  |  |  |
| Spare tyre or wheel/s are secured to carrier by secondary restraint (where spare tyre or wheel is carried). |  |  |  |
| Secondary restraints are used to secure sundry loose items or other items that are not stored in secured cabinets that can move in transit before the vehicle travels on a mine or public or private road. |  |  |  |

# Supervisor Task Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Verify fitted secondary restraint systems are used to secure equipment that can move in transit. |  |  |  |
| Verify other sundry loose items that can move in transit are secured as per load restraint procedures. |  |  |  |

# Operator / Maintainer Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Inspect condition of restraint equipment before use, repair or report damaged equipment. |  |  |  |
| Secure fitted secondary restraints to ensure all equipment that can move is secured in the home position before travelling on a public, private or mine roads. |  |  |  |
| Fit secondary restraints as per load restraint procedures to secure sundry loose support items or other items that can move (that are not stored in secured cabinets) in transit before travelling on a public, private or mine roads. |  |  |  |
| Check all equipment, items and cabinets are secure before moving off. |  |  |  |

# Comments/Actions