|  |  |
| --- | --- |
| Working At Hight On Vehicles Or Mobile Equipment |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name:** |  | **Date:** |  |
| **Job Description:** |  | **Location:** |  |

# Performance Metrics

|  |  |  |  |
| --- | --- | --- | --- |
|  | ✓ | 🗶 | • |
| Fixed platforms, walkways, stairways and handrails on mobile equipment and vehicles are designed to support people safely in accordance with recognised standards. |  |  |  |
| Isolations preventing movement of the mobile equipment or vehicle are checked and verified before work commences from an elevated position. |  |  |  |
| Drivers of mobile equipment or vehicles on site are trained, including holding any licence or permit required by local regulations. |  |  |  |
| People working in an elevated position on mobile equipment or vehicles are trained and assessed as competent in working at heights, including fall protection. |  |  |  |
| Parking procedures are in place, and followed, for all mobile equipment and vehicles requiring access by a person in an elevated position. |  |  |  |
| An exclusion zone is established around the mobile equipment or vehicle, including barricades, signs and an observer, to prevent third party access. |  |  |  |
| Drivers of mobile equipment and vehicles requiring access by a person in an elevated position are trained in the parking and isolation requirements. |  |  |  |
| Fall protection equipment, consisting of a harness and fixed-length lanyard (or other approved fall prevention system), is worn and attached to an approved anchor point whilst working in an unprotected elevated position on mobile equipment or vehicles. |  |  |  |

# Supervisor Task Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Verify any mobile equipment or vehicle, requiring work from an elevated position, is fitted with an approved anchor point. |  |  |  |
| Verify parking and isolation procedures are in place for all mobile equipment and vehicles that require access by a person in an elevated position. |  |  |  |
| Verify that any person required to work in an elevated position on mobile equipment is trained and assessed competent in working at heights. |  |  |  |

# Operator / Maintainer Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Park and isolate the mobile equipment or vehicle in accordance with procedures. |  |  |  |
| Establish an exclusion zone around the mobile equipment or vehicle, including barricades, signs and an observer, before accessing the work area. |  |  |  |
| Work in an elevated position on mobile equipment only if trained in working at heights. Do not proceed with work if not trained. |  |  |  |
| Wear fall protection equipment attached to an approved anchor point when working in an unprotected elevated position on mobile equipment or vehicles. |  |  |  |

# Comments/Actions