|  |  |
| --- | --- |
| Operating Vehicles and Mobile Equipment  On-site - Pedestrian and Site Requirements |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name:** |  | **Date:** |  |
| **Job Description:** |  | **Location:** |  |

# Performance Metrics

|  |  |  |  |
| --- | --- | --- | --- |
|  | ✓ | 🗶 | • |
| Pedestrian walkways are physically separated from operating vehicles and mobile equipment (e.g. barricades, raised walkway, distance of 3 metres or more etc.), and clearly marked. |  |  |  |
| Pedestrian crossings are designated, clearly marked, and illuminated if used outside daylight hours. Pedestrians have right-of-way at crossings. |  |  |  |
| Pedestrians wear Hi-Viz clothing when departing from designated walkways and crossings in areas of mixed pedestrian and vehicle occupation, or wherever required by site rules. |  |  |  |
| Exclusion zones for vehicles, mobile equipment and pedestrians are defined, clearly marked and enforced. |  |  |  |
| Vehicle and mobile equipment routes are designated and signposted. |  |  |  |
| Speed limits are set, signposted and enforced, and restricted to walking pace in areas of mixed pedestrian and vehicle occupation. |  |  |  |
| Areas of restricted vision (e.g. blind spots, building entries with mixed occupation etc.) are identified and controls put in place (e.g. mirrors, barriers etc.). |  |  |  |
| When pedestrians are required to enter an area where mobile equipment is operating, consent is first obtained from the mobile equipment driver. |  |  |  |

# Supervisor Task Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Provide designated, marked walkways and pedestrian crossings. |  |  |  |
| Provide designated, signposted vehicle and mobile equipment routes. |  |  |  |
| Set speed limits for site and provide signposting. |  |  |  |
| Define exclusion zones for vehicles, mobile equipment and pedestrians and provide signage. |  |  |  |
| Identify areas of restricted vision (e.g. blind spots, building entries with mixed occupation etc.) and provide controls (e.g. mirrors, barriers etc.). |  |  |  |
| Provide Hi-Viz clothing for site personnel and visitors. |  |  |  |
| Verify that assets protecting against vehicle, mobile equipment and pedestrian interactions (e.g. signage, markings, lighting, mirrors, barricading etc.) have been maintained in accordance with the established program. |  |  |  |

# Operator / Maintainer Requirements

|  |  |  |  |
| --- | --- | --- | --- |
| Use designated walkways and crossings when walking around site. |  |  |  |
| Do not enter pedestrian exclusion zones. |  |  |  |
| Wear Hi-Viz clothing in designated areas. |  |  |  |
| Obtain consent from the driver before entering an area where mobile equipment is operating. |  |  |  |

|  |  |
| --- | --- |
| Operating Vehicles and Mobile Equipment  On-site - Pedestrian and Site Requirements |  |

# Comments/Actions